{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet0"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Sheet0","index":0,"n_rows":3,"n_cols":8,"rows_kept":3,"merged":[[0,0,0,7]]}
["任务台账"]
["序号","检查对象","所属区县","任务类型","执法人员","检查时间","是否发现问题","检查情况"]
["1","河源市正天检测有限公司","源城区","双随机/监测机构","朱祖其、谢小平、陈港\n（河源生态环境监测站专家协助）","2025-7-25","发现一般问题","现场检查情况：\n1.移液枪EM0237，未及时校准；\n2.报告（编号：202502048）：报告原始记录中样品接样时间和分析时间未具体到小时，无法判断短期保质期样品的有效性；样品交接流转记录交接时间与COD和PH原始记录分析表中交接时间不一致；分析仪器没有编号，没有唯一性记录，无法溯源；PH样品分析超过样品2小时保质期。\n3.报告（编号：202412158）： 报告的流量测量原始记录，引用方法有误。                               针对上述问题，已现场要求企业整改。"]