{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["废气排放","废水排放"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"废气排放","index":0,"n_rows":5,"n_cols":24,"rows_kept":5,"merged":[[1,0,4,0],[1,1,4,1]],"flags":["formulas_cached_only"]}
["任务名称","企业名称","名录类别","行业类别","执行标准名称","执行标准条目名称","监测点","监测项目","监测日期","流量(m³/h)","温度(°C)","湿度(%)","含氧量(%)","流速(m/s)","生产负荷(%)","实测浓度","折算浓度","上限","下限","单位","是否超标","超标倍数","备注","是否有评价限值"]
["2023年第1季度电厂监督性监测","深能合和电力（河源）有限公司","大气环境","火力发电","火电厂大气污染物排放标准(GB13223-2011)","（表2）大气污染物特别排放限值,烟囱或烟道,燃煤锅炉","烟囱总排放口(DA001)","氮氧化物","2023-02-15","","","","","","","22","28","100","","mg/m3","否","","","是"]
["2023年第1季度电厂监督性监测","深能合和电力（河源）有限公司","大气环境","火力发电","火电厂大气污染物排放标准(GB13223-2011)","（表1）火力发电锅炉及燃汽轮机组大气污染物排放浓度限值,烟囱或烟道,燃煤锅炉,现有锅炉","烟囱总排放口(DA001)","二氧化硫","2023-02-15","","","","","","","<3","<3","200","","mg/m3","否","","","是"]
["2023年第1季度电厂监督性监测","深能合和电力（河源）有限公司","大气环境","火力发电","火电厂大气污染物排放标准(GB13223-2011)","（表2）大气污染物特别排放限值,烟囱或烟道,燃煤锅炉","烟囱总排放口(DA001)","汞及其化合物","2023-02-15","","","","","","","<0.0025","<0.0025","0.03","","mg/Nm3","否","","","是"]
["2023年第1季度电厂监督性监测","深能合和电力（河源）有限公司","大气环境","火力发电","火电厂大气污染物排放标准(GB13223-2011)","（表1）火力发电锅炉及燃汽轮机组大气污染物排放浓度限值,烟囱或烟道,燃煤锅炉,全部,通用","烟囱总排放口(DA001)","烟尘","2023-02-15","","","","","","","<1.0","<1.0","30","","mg/m3","否","","","是"]

{"sheet":"废水排放","index":1,"n_rows":73,"n_cols":22,"rows_kept":73,"merged":[[1,0,72,0],[1,1,18,1],[19,1,36,1],[37,1,54,1],[55,1,72,1]],"flags":["formulas_cached_only"]}
["任务名称","企业名称","名录类别","行业类别","受纳水体","执行标准名称","执行标准条目名称","监测点","监测项目","监测日期","流量(m³/s)","水温(°C)","生产负荷(%)","进口浓度","排放浓度","上限","下限","单位","是否超标","超标倍数","备注","是否有评价限值"]
["2023年第1季度重点污染源监督性监测","河源市广业环保有限公司河源市源城污水处理厂","水环境","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施出水口(WS-00061)","五日生化需氧量","2023-01-28","","","","","1.5","4","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市广业环保有限公司河源市源城污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00061)","悬浮物","2023-01-28","","","","","4","10","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市广业环保有限公司河源市源城污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00061)","总铬","2023-01-28","","","","","<0.004","0.1","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市广业环保有限公司河源市源城污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00061)","色度","2023-01-28","","","","","2","30","","倍","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市广业环保有限公司河源市源城污水处理厂","水环境","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施出水口(WS-00061)","镉","2023-01-28","","","","","<0.00005","0.005","","mg/KG","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市广业环保有限公司河源市源城污水处理厂","水环境","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施出水口(WS-00061)","石油类","2023-01-28","","","","","<0.06","0.05","","mg/KG","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市广业环保有限公司河源市源城污水处理厂","水环境","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施出水口(WS-00061)","汞","2023-01-28","","","","","<0.00004","0.0001","","mg/m3","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市广业环保有限公司河源市源城污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00061)","阴离子表面活性剂（LAS）","2023-01-28","","","","","0.034","0.5","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市广业环保有限公司河源市源城污水处理厂","水环境","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施出水口(WS-00061)","pH值","2023-01-28","","","","","7.6","9","6","无量纲","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市广业环保有限公司河源市源城污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00061)","六价铬","2023-01-28","","","","","<0.004","0.05","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市广业环保有限公司河源市源城污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00061)","动植物油","2023-01-28","","","","","<0.06","1","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市广业环保有限公司河源市源城污水处理厂","水环境","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施出水口(WS-00061)","化学需氧量","2023-01-28","","","","","<4","20","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市广业环保有限公司河源市源城污水处理厂","水环境","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施出水口(WS-00061)","砷","2023-01-28","","","","","0.00084","0.05","","mg/KG","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市广业环保有限公司河源市源城污水处理厂","水环境","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施出水口(WS-00061)","铅","2023-01-28","","","","","0.00020","0.05","","mg/Nm3","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市广业环保有限公司河源市源城污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00061)","氨氮（NH3-N）","2023-01-28","","","","","<0.025","1.0","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市广业环保有限公司河源市源城污水处理厂","水环境","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施出水口(WS-00061)","总磷（以P计）","2023-01-28","","","","","<0.01","0.2","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市广业环保有限公司河源市源城污水处理厂","水环境","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施出水口(WS-00061)","粪大肠菌群数","2023-01-28","","","","","500","10000","","个/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市广业环保有限公司河源市源城污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂水污染物排放标准(DB11/890-2012)(DB11/890-2012)","污水厂","废水处理设施出水口(WS-00061)","总氮（以N计）","2023-01-28","","","","","3.18","15","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市市区城南污水处理厂","","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施(DW001)","石油类","2023-01-28","","","","","<0.06","0.05","","mg/KG","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市市区城南污水处理厂","","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施(DW001)","砷","2023-01-28","","","","","0.00114","0.05","","mg/KG","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市市区城南污水处理厂","","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施(DW001)","汞","2023-01-28","","","","","<0.00004","0.0001","","mg/m3","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市市区城南污水处理厂","","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施(DW001)","氨氮（NH3-N）","2023-01-28","","","","","0.334","1.0","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市市区城南污水处理厂","","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施(DW001)","铅","2023-01-28","","","","","0.00135","0.05","","mg/Nm3","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市市区城南污水处理厂","","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施(DW001)","化学需氧量","2023-01-28","","","","","14","20","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市市区城南污水处理厂","","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施(DW001)","六价铬","2023-01-28","","","","","<0.004","0.05","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市市区城南污水处理厂","","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施(DW001)","阴离子表面活性剂（LAS）","2023-01-28","","","","","0.026","0.2","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市市区城南污水处理厂","","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施(DW001)","五日生化需氧量","2023-01-28","","","","","3.5","4","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市市区城南污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施(DW001)","总镉","2023-01-28","","","","","<0.00005","0.005","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市市区城南污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施(DW001)","动植物油","2023-01-28","","","","","<0.06","1","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市市区城南污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水处理设施(DW001)","色度","2023-01-28","","","","","2","30","","倍","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市市区城南污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水处理设施(DW001)","粪大肠菌群数","2023-01-28","","","","","300","10000","","个/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市市区城南污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施(DW001)","pH值","2023-01-28","","","","","7.5","9","6","无量纲","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市市区城南污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施(DW001)","悬浮物","2023-01-28","","","","","7","10","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市市区城南污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施(DW001)","总铬","2023-01-28","","","","","<0.004","0.1","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市市区城南污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施(DW001)","总氮（以N计）","2023-01-28","","","","","4.74","15","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市市区城南污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,2006年1月1日后建设","废水处理设施(DW001)","总磷（以P计）","2023-01-28","","","","","0.04","0.2","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","紫金县古竹污水处理厂","","污水处理及其再生利用","","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,城镇二级污水处理厂","废水处理设施出水口(WS-00099)","化学需氧量","2023-04-07","","","","","12","40","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","紫金县古竹污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00099)","总镉","2023-04-07","","","","","<0.00005","0.01","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","紫金县古竹污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00099)","石油类","2023-04-07","","","","","<0.06","1","","mg/KG","否","","","是"]
["2023年第1季度重点污染源监督性监测","紫金县古竹污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00099)","动植物油","2023-04-07","","","","","<0.06","1","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","紫金县古竹污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00099)","氨氮（NH3-N）","2023-04-07","","","","","0.331","5;8","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","紫金县古竹污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00099)","总汞","2023-04-07","","","","","<0.00004","1","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","紫金县古竹污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00099)","色度","2023-04-07","","","","","2","30","","倍","否","","","是"]
["2023年第1季度重点污染源监督性监测","紫金县古竹污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00099)","六价铬","2023-04-07","","","","","<0.004","0.05","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","紫金县古竹污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00099)","阴离子表面活性剂（LAS）","2023-04-07","","","","","0.033","0.5","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","紫金县古竹污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00099)","总砷","2023-04-07","","","","","0.00090","0.1","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","紫金县古竹污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00099)","粪大肠菌群数","2023-04-07","","","","","300","1000","","个/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","紫金县古竹污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00099)","pH值","2023-04-07","","","","","7.8","9","6","无量纲","否","","","是"]
["2023年第1季度重点污染源监督性监测","紫金县古竹污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00099)","总铅","2023-04-07","","","","","0.00094","0.1","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","紫金县古竹污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00099)","悬浮物","2023-04-07","","","","","5","10","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","紫金县古竹污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00099)","总铬","2023-04-07","","","","","<0.004","0.1","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","紫金县古竹污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00099)","总氮（以N计）","2023-04-07","","","","","4.40","15","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","紫金县古竹污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,2006年1月1日后建设","废水处理设施出水口(WS-00099)","总磷（以P计）","2023-04-07","","","","","0.03","0.5","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","紫金县古竹污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00099)","五日生化需氧量","2023-04-07","","","","","2.6","10","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),一级标准,城镇二级污水处理厂","废水处理设施出水口(WS—00043)","化学需氧量","2023-04-07","","","","","10","40","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水处理设施出水口(WS—00043)","总镉","2023-04-07","","","","","<0.00005","0.01","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水处理设施出水口(WS—00043)","石油类","2023-04-07","","","","","<0.06","3","","mg/KG","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水处理设施出水口(WS—00043)","动植物油","2023-04-07","","","","","<0.06","3","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水处理设施出水口(WS—00043)","氨氮（NH3-N）","2023-04-07","","","","","7.00","8;15","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水处理设施出水口(WS—00043)","总汞","2023-04-07","","","","","<0.00004","0.001","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水处理设施出水口(WS—00043)","色度","2023-04-07","","","","","2","30","","倍","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水处理设施出水口(WS—00043)","六价铬","2023-04-07","","","","","<0.004","0.05","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水处理设施出水口(WS—00043)","阴离子表面活性剂（LAS）","2023-04-07","","","","","0.041","1","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水处理设施出水口(WS—00043)","总砷","2023-04-07","","","","","0.00225","0.1","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水处理设施出水口(WS—00043)","粪大肠菌群数","2023-04-07","","","","","200","10000","","个/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水处理设施出水口(WS—00043)","pH值","2023-04-07","","","","","7.0","9","6","无量纲","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水处理设施出水口(WS—00043)","总铅","2023-04-07","","","","","0.00060","0.1","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水处理设施出水口(WS—00043)","悬浮物","2023-04-07","","","","","10","20","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水处理设施出水口(WS—00043)","总铬","2023-04-07","","","","","<0.004","0.1","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水处理设施出水口(WS—00043)","总氮（以N计）","2023-04-07","","","","","10.9","20","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,2005年12月31日前建设","废水处理设施出水口(WS—00043)","总磷（以P计）","2023-04-07","","","","","0.51","1.5","","mg/L","否","","","是"]
["2023年第1季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水处理设施出水口(WS—00043)","五日生化需氧量","2023-04-07","","","","","2.1","20","","mg/L","否","","","是"]