{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":217,"n_cols":12,"rows_kept":217,"merged":[[0,0,0,1],[0,2,0,10],[2,0,24,0],[2,1,2,11],[3,1,3,11],[4,1,4,11],[5,1,5,11],[7,1,24,1],[7,2,24,2],[7,3,24,3],[7,4,24,4],[25,0,47,0],[25,1,25,11],[26,1,26,11],[27,1,27,11],[28,1,28,11],[29,8,29,9],[30,1,47,1],[30,2,47,2],[30,3,47,3],[30,4,47,4],[30,8,30,9],[31,8,31,9],[32,8,32,9],[33,8,33,9],[34,8,34,9],[35,8,35,9],[36,8,36,9],[37,8,37,9],[38,8,38,9],[39,8,39,9],[40,8,40,9],[41,8,41,9],[42,8,42,9],[43,8,43,9],[44,8,44,9],[45,8,45,9],[46,8,46,9],[47,8,47,9],[48,0,70,0],[48,1,48,11],[49,1,49,11],[50,1,50,11],[51,1,51,11],[53,1,70,1],[53,2,70,2],[53,3,70,3],[53,4,70,4],[71,0,95,0],[71,1,71,11],[72,1,72,11],[73,1,73,11],[74,1,74,11],[75,10,75,11],[76,1,95,1],[76,2,95,2],[76,3,95,3],[76,4,95,4],[76,10,95,11],[96,0,120,0],[96,1,96,11],[97,1,97,11],[98,1,98,11],[99,1,99,11],[100,10,100,11],[101,1,120,1],[101,2,120,2],[101,3,120,3],[101,4,120,4],[101,10,120,11],[121,0,143,0],[121,1,121,11],[122,1,122,11],[123,1,123,11],[124,1,124,11],[125,10,125,11],[126,1,143,1],[126,2,143,2],[126,3,143,3],[126,4,143,4],[126,10,143,11],[144,0,167,0],[144,1,144,11],[145,1,145,11],[146,1,146,11],[147,1,147,11],[148,8,148,9],[149,1,167,1],[149,2,167,2],[149,3,167,3],[149,4,167,4],[149,8,149,9],[149,11,167,11],[150,8,150,9],[151,8,151,9],[152,8,152,9],[153,8,153,9],[154,8,154,9],[155,8,155,9],[156,8,156,9],[157,8,157,9],[158,8,158,9],[159,8,159,9],[160,8,160,9],[161,8,161,9],[162,8,162,9],[163,8,163,9],[164,8,164,9],[165,8,165,9],[166,8,166,9],[167,8,167,9],[168,0,192,0],[168,1,168,11],[169,1,169,11],[170,1,170,11],[171,1,171,11],[172,8,172,9],[173,1,192,1],[173,2,192,2],[173,3,192,3],[173,4,192,4],[173,8,173,9],[173,11,192,11],[174,8,174,9],[175,8,175,9],[176,8,176,9],[177,8,177,9],[178,8,178,9],[179,8,179,9],[180,8,180,9],[181,8,181,9],[182,8,182,9],[183,8,183,9],[184,8,184,9],[185,8,185,9],[186,8,186,9],[187,8,187,9],[188,8,188,9],[189,8,189,9],[190,8,190,9],[191,8,191,9],[192,8,192,9],[193,0,216,0],[193,1,193,11],[194,1,194,11],[195,1,195,11],[196,1,196,11],[197,8,197,9],[198,1,216,1],[198,2,216,2],[198,3,216,3],[198,4,216,4],[198,8,198,9],[198,11,216,11],[199,8,199,9],[200,8,200,9],[201,8,201,9],[202,8,202,9],[203,8,203,9],[204,8,204,9],[205,8,205,9],[206,8,206,9],[207,8,207,9],[208,8,208,9],[209,8,209,9],[210,8,210,9],[211,8,211,9],[212,8,212,9],[213,8,213,9],[214,8,214,9],[215,8,215,9],[216,8,216,9]],"flags":["formulas_cached_only"]}
["附件2",null,"河源市2021年第1季度重点污染源监督性监测结果表（9家）"]
["序号"]
[1,"企业名称：河源市市区城南污水处理厂"]
[null,"企业类型：其他企业"]
[null,"详细地址：河源市高新区科技九路"]
[null,"监测单位：河源市环境监测站"]
[null,"类型","监测点位","监测日期","执行标准","污染因子","排放浓度","单位","标准限值","参照执行标准","达标情况","未开展监测的原因"]
[null,"污水处理厂","出水口","2021-01-06","执行《地表水环境质量标准》（GB3838-2002）表1地表水环境质量标准基本项目标准限值Ⅲ类标准值；GB3838-2002表1中无控制标准因子参照执行《城镇污水处理厂污染物排放标准》（GB1891-2002）表1基本控制项目最高允许排放浓度一级标准A限值或表3选择控制项目最高允许排放浓度。","pH值",6.87,"无量钢","6--9","—","达标"]
[{"$nulls":5},"色度（倍）","<2","倍","─",30,"达标"]
[{"$nulls":5},"悬浮物","<4"," mg/L","─",10,"达标"]
[{"$nulls":5},"化学需氧量",7," mg/L",20,"—","达标"]
[{"$nulls":5},"五日生化需氧量",1.7," mg/L",4,"—","达标"]
[{"$nulls":5},"氨氮",0.185," mg/L",1,"—","达标"]
[{"$nulls":5},"总磷",0.02,"mg/L",0.2,"—","达标"]
[{"$nulls":5},"总氮",5.61,"mg/L","—",15,"达标"]
[{"$nulls":5},"动植物油","<0.06","mg/L","─",1,"达标"]
[{"$nulls":5},"石油类","<0.01","mg/L",0.05,"─","达标"]
[{"$nulls":5},"阴离子表面活性剂","<0.05","mg/L ",0.2,"—","达标"]
[{"$nulls":5}," 粪大肠菌群",6750," 个/L",10000,"—","达标"]
[{"$nulls":5},"总汞","<0.00004","mg/L",0.0001,"—","达标"]
[{"$nulls":5},"总砷",0.0009,"mg/L",0.05,"—","达标"]
[{"$nulls":5},"总铬","<0.004","mg/L","─","—","达标"]
[{"$nulls":5},"总镉","<0.00006","mg/L",0.005,"—","达标"]
[{"$nulls":5},"总铅","<0.00007","mg/L",0.05,"—","达标"]
[{"$nulls":5},"六价铬","<0.004","mg/L",0.05,"—","达标"]
[2,"企业名称：河源市污水处理厂 "]
[null,"企业类型：其他企业"]
[null,"详细地址：河源市源城区龙王阁"]
[null,"监测单位：河源市环境监测站"]
[null,"类型","监测点位","监测日期","执行标准","污染因子","排放浓度","单位","标准限值",null,"达标情况","未开展监测的原因"]
[null,"污水处理厂","出水口","2021-01-12","《水污染物排放限值》（DB44/26-2001）第二时段一级标准和《城镇污水处理厂污染物排放标准》（GB18918-2002）一级B标准中的较严者","pH值",7.18,"无量钢","6--9",null,"达标"]
[{"$nulls":5},"色度（倍）","<2","倍",30,null,"达标"]
[{"$nulls":5},"悬浮物",9," mg/L",20,null,"达标"]
[{"$nulls":5},"化学需氧量",13," mg/L",40,null,"达标"]
[{"$nulls":5},"五日生化需氧量",2.8," mg/L",20,null,"达标"]
[{"$nulls":5},"氨氮",2.24," mg/L",8,null,"达标"]
[{"$nulls":5},"总磷",0.74,"mg/L",1.5,null,"达标"]
[{"$nulls":5},"总氮",8.55,"mg/L ",20,null,"达标"]
[{"$nulls":5},"石油类","<0.06","mg/L ",3,null,"达标"]
[{"$nulls":5},"动植物油","<0.06","mg/L ",3,null,"达标"]
[{"$nulls":5},"阴离子表面活性剂","<0.05","mg/L ",1,null,"达标"]
[{"$nulls":5}," 粪大肠菌群",3750," 个/L",10000,null,"达标"]
[{"$nulls":5},"总汞","<0.00004","mg/L ",0.001,null,"达标"]
[{"$nulls":5},"总砷",0.0017,"mg/L",0.1,null,"达标"]
[{"$nulls":5},"总铬","<0.004","mg/L",0.1,null,"达标"]
[{"$nulls":5},"总镉","<0.00006","mg/L",0.01,null,"达标"]
[{"$nulls":5},"总铅","<0.00007","mg/L ",0.1,null,"达标"]
[{"$nulls":5},"六价铬","<0.004","mg/L ",0.05,null,"达标"]
[3,"企业名称：河源市广业环保有限公司(河源市源城污水处理厂)"]
[null,"企业类型：其他企业"]
[null,"详细地址：河源市源城区埔前镇莲塘岭大简"]
[null,"监测单位：河源市环境监测站"]
[null,"类型","监测点位","监测日期","执行标准","污染因子","排放浓度","单位","标准限值","参照执行标准","达标情况","未开展监测的原因"]
[null,"污水处理厂","出水口","2021-01-05","执行《地表水环境质量标准》（GB3838-2002）表1地表水环境质量标准基本项目标准限值Ⅲ类标准值；GB3838-2002表1中无控制标准因子参照执行《城镇污水处理厂污染物排放标准》（GB1891-2002）表1基本控制项目最高允许排放浓度一级标准A限值；","pH值",7.19,"无量钢","6--9","—","达标"]
[{"$nulls":5},"色度（倍）","<2","倍","—",30,"达标"]
[{"$nulls":5},"悬浮物","<4"," mg/L","—",10,"达标"]
[{"$nulls":5},"化学需氧量","<4"," mg/L",20,"—","达标"]
[{"$nulls":5},"五日生化需氧量",1.2," mg/L",4,"—","达标"]
[{"$nulls":5},"氨氮",0.051," mg/L",1,"—","达标"]
[{"$nulls":5},"总磷",0.02,"mg/L",0.2,"—","达标"]
[{"$nulls":5},"总氮",2.19,"mg/L","—",15,"达标"]
[{"$nulls":5},"动植物油","<0.06","mg/L",0.05,"—","达标"]
[{"$nulls":5},"石油类","<0.01","mg/L",0.05,"—","达标"]
[{"$nulls":5},"阴离子表面活性剂","<0.05","mg/L ",0.2,"—","达标"]
[{"$nulls":5}," 粪大肠菌群",7500," 个/L",10000,"—","达标"]
[{"$nulls":5},"总汞","<0.00004","mg/L",0.0001,"—","达标"]
[{"$nulls":5},"总砷",0.0005,"mg/L",0.05,"—","达标"]
[{"$nulls":5},"总铬","<0.004","mg/L","—","—","达标"]
[{"$nulls":5},"总镉","<0.00006","mg/L",0.005,"—","达标"]
[{"$nulls":5},"总铅","<0.00007","mg/L",0.05,"—","达标"]
[{"$nulls":5},"六价铬","<0.004","mg/L",0.05,"—","达标"]
[4,"企业名称：连平县生活污水处理厂"]
[null,"企业类型：其他企业"]
[null,"详细地址：河源市连平县元善镇天后娘"]
[null,"监测单位：连平县环境监测站"]
[null,"类型","监测点位","监测日期","执行标准","污染因子","排放浓度","单位","标准限值","达标情况","未开展监测的原因"]
[null,"污水处理厂","出水口","2021-01-08","《水污染物排放限值》（DB44/26-2001）第二时段一级标准和《城镇污水处理厂污染物排放标准》（GB18918-2002）一级B标准中的较严者","pH值",6.95,"无量钢","6--9","达标"]
[{"$nulls":5},"色度（倍）",2,"倍",30,"达标"]
[{"$nulls":5},"悬浮物",10," mg/L",20,"达标"]
[{"$nulls":5},"化学需氧量",20," mg/L",40,"达标"]
[{"$nulls":5},"五日生化需氧量",4.6," mg/L",20,"达标"]
[{"$nulls":5},"氨氮",4.837," mg/L",8,"达标"]
[{"$nulls":5},"总磷",0.34,"mg/L",0.5,"达标"]
[{"$nulls":5},"总氮",10.12,"mg/L",20,"达标"]
[{"$nulls":5},"六价铬","<0.004","mg/L",0.05,"达标"]
[{"$nulls":5},"总铬","<0.03","mg/L",0.1,"达标"]
[{"$nulls":5},"砷",0.0014,"mg/L",0.1,"达标"]
[{"$nulls":5},"汞","<0.00004","mg/L",0.001,"达标"]
[{"$nulls":5},"总镉","<0.0025","mg/L",0.01,"达标"]
[{"$nulls":5},"总铅","<0.005","mg/L",0.1,"达标"]
[{"$nulls":5},"粪大肠菌群",2100,"（个/L）",10000,"达标"]
[{"$nulls":5},"阴离子表面活性剂",0.06,"mg/L",1,"达标"]
[{"$nulls":5},"石油类","<0.06","mg/L ",3,"达标"]
[{"$nulls":5},"动植物油","<0.06"," 个/L",3,"达标"]
[{"$nulls":5},"甲基汞","<0.00001","mg/L ","不得检出","达标"]
[{"$nulls":5},"乙基汞","<0.00002","mg/L ","不得检出","达标"]
[5,"企业名称：河源市广业环保有限公司龙川县城生活污水处理厂"]
[null,"企业类型：其他企业"]
[null,"详细地址：河源市龙川县老隆镇涧洞村"]
[null,"监测单位：龙川县环境监测站"]
[null,"类型","监测点位","监测日期","执行标准","污染因子","排放浓度","单位","标准限值","达标情况","未开展监测的原因"]
[null,"污水处理厂","出水口","2021-01-20","《水污染物排放限值》（DB44/26-2001）第二时段一级标准和《城镇污水处理厂污染物排放标准》（GB18918-2002）一级A标准中的较严者","pH值",6.77,"无量钢","6--9","达标"]
[{"$nulls":5},"色度（倍）",16,"倍",30,"达标"]
[{"$nulls":5},"悬浮物",8," mg/L",10,"达标"]
[{"$nulls":5},"化学需氧量",23," mg/L",50,"达标"]
[{"$nulls":5},"五日生化需氧量",3.3," mg/L",10,"达标"]
[{"$nulls":5},"氨氮",1.91," mg/L",5,"达标"]
[{"$nulls":5},"总磷",0.14," mg/L",0.5,"达标"]
[{"$nulls":5},"总氮",{"v":9.3,"d":"9.30"}," mg/L",15,"达标"]
[{"$nulls":5},"石油类","＜0.06"," mg/L",1,"达标"]
[{"$nulls":5},"动植物油",0.09," mg/L",1,"达标"]
[{"$nulls":5},"阴离子表面活性剂",0.19," mg/L",0.5,"达标"]
[{"$nulls":5},"总汞","＜0.00002"," mg/L",0.001,"达标"]
[{"$nulls":5},"总镉","＜0.001","mg/L",0.01,"达标"]
[{"$nulls":5},"总铅","＜0.01","mg/L",0.1,"达标"]
[{"$nulls":5},"六价铬","＜0.004","mg/L",0.05,"达标"]
[{"$nulls":5}," 粪大肠菌群",640," 个/L",1000,"达标"]
[{"$nulls":5},"总铬","<0.03","mg/L ",0.1,"达标"]
[{"$nulls":5},"总砷",0.0019,"mg/L ",0.1,"达标"]
[{"$nulls":5},"甲基汞","<0.00001","mg/L ","不得检出","达标"]
[{"$nulls":5},"乙基汞","<0.00002","mg/L ","不得检出","达标"]
[6,"企业名称：紫金县古竹污水处理厂 "]
[null,"企业类型：其他企业"]
[null,"河源市紫金古竹镇"]
[null,"监测单位：河源市环境监测站"]
[null,"类型","监测点位","监测日期","执行标准","污染因子","排放浓度","单位","标准限值","达标情况","未开展监测的原因"]
[null,"污水处理厂","出水口","2021-01-04","《水污染物排放限值》（DB44/26-2001）第二时段一级标准和《城镇污水处理厂污染物排放标准》（GB18918-2002）一级A标准中的较严者","pH值",6.71,"无量钢","6--9","达标"]
[{"$nulls":5},"色度（倍）",2,"倍",30,"达标"]
[{"$nulls":5},"悬浮物",9," mg/L",10,"达标"]
[{"$nulls":5},"化学需氧量",9," mg/L",40,"达标"]
[{"$nulls":5},"五日生化需氧量",2.5," mg/L",10,"达标"]
[{"$nulls":5},"氨氮",0.267," mg/L",5,"达标"]
[{"$nulls":5},"总磷",0.07,"mg/L",0.5,"达标"]
[{"$nulls":5},"总氮",5.71,"mg/L",15,"达标"]
[{"$nulls":5},"石油类","<0.06","mg/L",1,"达标"]
[{"$nulls":5},"动植物油","<0.06","mg/L",1,"达标"]
[{"$nulls":5},"阴离子表面活性剂","<0.05","mg/L ",0.5,"达标"]
[{"$nulls":5}," 粪大肠菌群",725," 个/L",1000,"达标"]
[{"$nulls":5},"总汞","<0.00004","mg/L",0.001,"达标"]
[{"$nulls":5},"总砷",0.0007,"mg/L",0.1,"达标"]
[{"$nulls":5},"总铬","<0.004","mg/L",0.1,"达标"]
[{"$nulls":5},"总镉","<0.00006","mg/L",0.01,"达标"]
[{"$nulls":5},"总铅","<0.00007","mg/L",0.1,"达标"]
[{"$nulls":5},"六价铬","<0.004","mg/L",0.05,"达标"]
[7,"企业名称：河源市广业环保有限公司(和平县城污水处理厂)"]
[null,"企业类型：其他企业"]
[null,"详细地址：河源市和平县城"]
[null,"监测单位：和平县环境监测站"]
[null,"类型","监测点位","监测日期","执行标准","污染因子","排放浓度","单位","标准限值",null,"达标情况","未开展监测的原因"]
[null,"污水处理厂","出水口","2021-03-03","《水污染物排放限值》（DB44/26-2001）第二时段一级标准和《城镇污水处理厂污染物排放标准》（GB18918-2002）一级A标准中的较严者","pH值",6.79,"无量钢","6--9",null,"达标"]
[{"$nulls":5},"色度（倍）","<2","倍",30,null,"达标"]
[{"$nulls":5},"悬浮物",3.3," mg/L",10,null,"达标"]
[{"$nulls":5},"化学需氧量",19," mg/L",40,null,"达标"]
[{"$nulls":5},"氨氮",0.286," mg/L",5,null,"达标"]
[{"$nulls":5},"总磷",0.09,"mg/L",0.5,null,"达标"]
[{"$nulls":5},"总氮",9.42,"mg/L",15,null,"达标"]
[{"$nulls":5},"阴离子表面活性剂","<0.05","mg/L ",0.5,null,"达标"]
[{"$nulls":5},"总铬","<0.03","mg/L",0.1,null,"达标"]
[{"$nulls":5},"总铅","<0.07","mg/L",0.1,null,"达标"]
[{"$nulls":5},"总镉","<0.005","mg/L",0.01,null,"达标"]
[{"$nulls":5},"总砷","<0.0003","mg/L",0.1,null,"达标"]
[{"$nulls":5},"总汞","<0.00004","mg/L",0.001,null,"达标"]
[{"$nulls":5},"六价铬","<0.004","mg/L",0.05,null,"达标"]
[{"$nulls":5},"烷基汞","未检出","mg/L","不得检出",null,"达标"]
[{"$nulls":5},"五日生化需氧量",2.5," mg/L",10,null,"达标"]
[{"$nulls":5}," 粪大肠菌群",490," 个/L",1000,null,"达标"]
[{"$nulls":5},"石油类","<0.06","mg/L",1,null,"达标"]
[{"$nulls":5},"动植物油","<0.06","mg/L",1,null,"达标"]
[8,"企业名称：河源市广业环保有限公司(东源县城污水处理厂)"]
[null,"企业类型：其他企业"]
[null,"详细地址：河源市东源县木京村黄竹沥"]
[null,"监测单位：东源县环境监测站"]
[null,"类型","监测点位","监测日期","执行标准","污染因子","排放浓度","单位","标准限值",null,"达标情况","未开展监测的原因"]
[null,"污水处理厂","出水口","2021-01-12","《水污染物排放限值》（DB44/26-2001）第二时段一级标准、《城镇污水处理厂污染物排放标准》（GB18918－2002）表1基本控制项目最高允许排放浓度一级标准A限值及《地表水环境质量标准》（GB3838-2002）Ⅳ类水体水质要求三者中较严者。","pH值",{"v":6.4,"d":"6.40"},"无量钢","6--9",null,"达标"]
[{"$nulls":5},"色度（倍）",10,"倍",30,null,"达标"]
[{"$nulls":5},"悬浮物",8," mg/L",10,null,"达标"]
[{"$nulls":5},"化学需氧量","<10"," mg/L",30,null,"达标"]
[{"$nulls":5},"五日生化需氧量",2," mg/L",6,null,"达标"]
[{"$nulls":5},"氨氮",0.218," mg/L",1.5,null,"达标"]
[{"$nulls":5},"总磷",{"v":0.1,"d":"0.10"},"mg/L",0.3,null,"达标"]
[{"$nulls":5},"总氮",1.19,"mg/L",15,null,"达标"]
[{"$nulls":5},"总铅","<0.00009","mg/L",0.05,null,"达标"]
[{"$nulls":5},"总镉","<0.00005","mg/L",0.005,null,"达标"]
[{"$nulls":5},"总砷",0.00012,"mg/L",0.1,null,"达标"]
[{"$nulls":5},"总汞","<0.00004","mg/L",0.001,null,"达标"]
[{"$nulls":5},"六价铬",0.004,"mg/L",0.05,null,"达标"]
[{"$nulls":5},"石油类","<0.06","mg/L",1,null,"达标"]
[{"$nulls":5},"动植物油","<0.06","mg/L",1,null,"达标"]
[{"$nulls":5},"阴离子表面活性剂","<0.05","mg/L ",0.5,null,"达标"]
[{"$nulls":5}," 粪大肠菌群","<10"," 个/L",1000,null,"达标"]
[{"$nulls":5},"总铬","<0.03","mg/L",0.1,null,"达标"]
[{"$nulls":5},"甲基汞","<0.00001","mg/L","不得检出",null,"达标"]
[{"$nulls":5},"乙基汞","<0.00002","mg/L","不得检出",null,"达标"]
[9,"企业名称：紫金县城区污水处理厂 "]
[null,"企业类型：其他企业"]
[null,"详细地址：河源市紫金县紫城镇"]
[null,"监测单位：紫金县环境监测站"]
[null,"类型","监测点位","监测日期","执行标准","污染因子","排放浓度","单位","标准限值",null,"达标情况","未开展监测的原因"]
[null,"污水处理厂","出水口","2021-01-05","《水污染物排放限值》（DB44/26-2001）第二时段一级标准和《城镇污水处理厂污染物排放标准》（GB18918-2002）一级B标准中的较严者","pH值",6.84,"无量钢","6--9",null,"达标"]
[{"$nulls":5},"色度（倍）",2,"倍",30,null,"达标"]
[{"$nulls":5},"悬浮物",5," mg/L",20,null,"达标"]
[{"$nulls":5},"化学需氧量",16," mg/L",40,null,"达标"]
[{"$nulls":5},"氨氮",3.25," mg/L",8,null,"达标"]
[{"$nulls":5},"总磷",0.41,"mg/L",0.5,null,"达标"]
[{"$nulls":5},"六价铬","<0.004","mg/L",0.05,null,"达标"]
[{"$nulls":5},"五日生化需氧量",8.5," mg/L",20,null,"达标"]
[{"$nulls":5},"总氮",8.64,"mg/L",20,null,"达标"]
[{"$nulls":5},"总汞",5e-05,"mg/L",0.001,null,"达标"]
[{"$nulls":5},"总镉","<0.001","mg/L",0.01,null,"达标"]
[{"$nulls":5},"总铬","<0.004","mg/L",0.1,null,"达标"]
[{"$nulls":5},"总砷",0.0013,"mg/L",0.1,null,"达标"]
[{"$nulls":5},"总铅","<0.01","mg/L",0.1,null,"达标"]
[{"$nulls":5},"石油类","<0.06","mg/L",3,null,"达标"]
[{"$nulls":5},"动植物油","<0.06","mg/L",3,null,"达标"]
[{"$nulls":5},"阴离子表面活性剂","<0.05","mg/L ",1,null,"达标"]
[{"$nulls":5}," 粪大肠菌群",880," 个/L",10000,null,"达标"]
[{"$nulls":5},"烷基汞","<0.00003","mg/L","不得检出",null,"达标"]