{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["废水排放","无组织","周边环境"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"废水排放","index":0,"n_rows":35,"n_cols":22,"rows_kept":35,"merged":[[1,0,34,0],[1,1,15,1],[16,1,34,1]],"flags":["formulas_cached_only"]}
["任务名称","企业名称","名录类别","行业类别","受纳水体","执行标准名称","执行标准条目名称","监测点","监测项目","监测日期","流量(m³/s)","水温(°C)","生产负荷(%)","进口浓度","排放浓度","上限","下限","单位","是否超标","超标倍数","备注","是否有评价限值"]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物特别排放限值","总排污口","总铬","2023-02-24","","","","","0.025","0.1","","mg/L","否","","","是"]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","总排污口","总铅","2023-02-24","","","","","<0.005","0.1","","mg/L","否","","","是"]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","总排污口","色度","2023-02-24","","","","","1","40","","倍","否","","","是"]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物特别排放限值","总排污口","粪大肠菌群数","2023-02-24","","","","","200","10000","","MPN/L","否","","","是"]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,其他排污单位","总排污口","化学需氧量","2023-02-24","","","","","12","90","","mg/L","否","","","是"]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,其他排污单位","总排污口","氨氮（NH3-N）","2023-02-24","","","","","0.529","10","","mg/L","否","","","是"]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","总排污口","悬浮物","2023-02-24","","","","","11","30","","mg/L","否","","","是"]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,一切排污单位","总排污口","pH值","2023-02-24","","","","","6.4","9","6","mg/L","否","","","是"]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,其他排污单位","总排污口","磷酸盐（以P计）","2023-02-24","","","","","<0.01","0.5","","mg/L","否","","","是"]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","总排污口","六价铬","2023-02-24","","","","","<0.004","0.05","","mg/L","否","","","是"]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","总排污口","总汞","2023-02-24","","","","","0.00008","0.001","","mg/L","否","","","是"]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","总排污口","总氮（以N计）","2023-02-24","","","","","2.28","40","","mg/L","否","","","是"]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","总排污口","总砷","2023-02-24","","","","","<0.0003","0.1","","mg/L","否","","","是"]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,其他排污单位","总排污口","五日生化需氧量","2023-02-24","","","","","3.6","20","","mg/L","否","","","是"]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","总排污口","总镉","2023-02-24","","","","","<0.0025","0.01","","mg/L","否","","","是"]
["2023年第一季度污染源监测","连平县生活污水处理厂","水环境","污水处理及其再生利用","连平河","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,四类,通用","总排放口(DW001)","六价铬","2023-01-10","","17","","","<0.004","0.05","","mg/L","否","","","是"]
["2023年第一季度污染源监测","连平县生活污水处理厂","水环境","污水处理及其再生利用","连平河","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","总排放口(DW001)","总镉","2023-01-10","","17","","","<0.0025","0.01","","mg/L","否","","","是"]
["2023年第一季度污染源监测","连平县生活污水处理厂","水环境","污水处理及其再生利用","连平河","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","总排放口(DW001)","总砷","2023-01-10","","17","","","<0.0003","0.1","","mg/L","否","","","是"]
["2023年第一季度污染源监测","连平县生活污水处理厂","水环境","污水处理及其再生利用","连平河","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","总排放口(DW001)","总铬","2023-01-10","","17","","","<0.03","0.1","","mg/L","否","","","是"]
["2023年第一季度污染源监测","连平县生活污水处理厂","水环境","污水处理及其再生利用","连平河","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","总排放口(DW001)","色度","2023-01-10","","17","","","2","30","","倍","否","","","是"]
["2023年第一季度污染源监测","连平县生活污水处理厂","水环境","污水处理及其再生利用","连平河","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,四类,通用","总排放口(DW001)","粪大肠菌群数","2023-01-10","","17","","","98","20000","","个/L","否","","","是"]
["2023年第一季度污染源监测","连平县生活污水处理厂","水环境","污水处理及其再生利用","连平河","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,四类,通用","总排放口(DW001)","石油类","2023-01-10","","17","","","0.33","0.5","","mg/L","否","","","是"]
["2023年第一季度污染源监测","连平县生活污水处理厂","水环境","污水处理及其再生利用","连平河","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","总排放口(DW001)","动植物油","2023-01-10","","17","","","0.10","1","","mg/L","否","","","是"]
["2023年第一季度污染源监测","连平县生活污水处理厂","水环境","污水处理及其再生利用","连平河","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","总排放口(DW001)","总铅","2023-01-10","","17","","","<0.005","0.05","","mg/L","否","","","是"]
["2023年第一季度污染源监测","连平县生活污水处理厂","水环境","污水处理及其再生利用","连平河","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","总排放口(DW001)","阴离子表面活性剂","2023-01-10","","17","","","<0.05","0.3","","mg/L","否","","","是"]
["2023年第一季度污染源监测","连平县生活污水处理厂","水环境","污水处理及其再生利用","连平河","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,四类,通用","总排放口(DW001)","氨氮（NH3-N）","2023-01-10","","17","","","0.545","1.5","","mg/L","否","","","是"]
["2023年第一季度污染源监测","连平县生活污水处理厂","水环境","污水处理及其再生利用","连平河","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,四类,通用","总排放口(DW001)","pH值","2023-01-10","","17","","","7.1","9","6","无量纲","否","","","是"]
["2023年第一季度污染源监测","连平县生活污水处理厂","水环境","污水处理及其再生利用","连平河","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","总排放口(DW001)","悬浮物","2023-01-10","","17","","","9","10","","mg/L","否","","","是"]
["2023年第一季度污染源监测","连平县生活污水处理厂","水环境","污水处理及其再生利用","连平河","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,四类,通用","总排放口(DW001)","总磷（以P计）","2023-01-10","","17","","","0.15","0.3","","mg/L","否","","","是"]
["2023年第一季度污染源监测","连平县生活污水处理厂","水环境","污水处理及其再生利用","连平河","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","总排放口(DW001)","总氮（以N计）","2023-01-10","","17","","","6.09","15","","mg/L","否","","","是"]
["2023年第一季度污染源监测","连平县生活污水处理厂","水环境","污水处理及其再生利用","连平河","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","总排放口(DW001)","总汞","2023-01-10","","17","","","<0.00004","0.001","","mg/L","否","","","是"]
["2023年第一季度污染源监测","连平县生活污水处理厂","水环境","污水处理及其再生利用","连平河","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","总排放口(DW001)","烷基汞","2023-01-10","","17","","","<0.00001","0.000010","","mg/L","否","","","是"]
["2023年第一季度污染源监测","连平县生活污水处理厂","水环境","污水处理及其再生利用","连平河","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,四类,通用","总排放口(DW001)","化学需氧量","2023-01-10","","17","","","13","30","","mg/L","否","","","是"]
["2023年第一季度污染源监测","连平县生活污水处理厂","水环境","污水处理及其再生利用","连平河","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,四类,通用","总排放口(DW001)","五日生化需氧量","2023-01-10","","17","","","3.3","6","","mg/L","否","","","是"]

{"sheet":"无组织","index":1,"n_rows":9,"n_cols":20,"rows_kept":9,"merged":[[1,0,8,0],[1,1,8,1]],"flags":["formulas_cached_only"]}
["任务名称","企业名称","名录类别","行业类别","执行标准名称","执行标准条目名称","监测点","监测项目","监测日期","风向","风速（m/s）","温度(℃)","压力（kPa）","排放浓度","上限","下限","单位","是否超标","超标倍数","备注"]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值,直接排放","北侧场界外4#","甲烷","2023-02-24","南","1.7","19.4","100.2","0.00348","0.1","","%","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","恶臭污染物排放标准(GB14554-93)","（表1）恶臭污染物厂界标准值,二级,新扩改建","北侧场界外4#","臭气浓度","2023-02-24","南","1.7","19.4","100.2","74","20","","无量纲","是","2.70",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值,直接排放","东侧场界外1#","甲烷","2023-02-24","南","1.8","19.3","100.3","0.000192","0.1","","%","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","恶臭污染物排放标准(GB14554-93)","（表1）恶臭污染物厂界标准值,二级,新扩改建","东侧场界外1#","臭气浓度","2023-02-24","南","1.8","19.3","100.3","<10","20","","无量纲","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值,直接排放","南侧场界外2#","甲烷","2023-02-24","南","1.6","19.5","100.5","0.000199","0.1","","%","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","恶臭污染物排放标准(GB14554-93)","（表1）恶臭污染物厂界标准值,二级,新扩改建","南侧场界外2#","臭气浓度","2023-02-24","南","1.6","19.5","100.5","<10","20","","无量纲","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值,直接排放","西侧场界外3#","甲烷","2023-02-24","南","1.6","19.6","100.3","0.0002","0.1","","%","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","恶臭污染物排放标准(GB14554-93)","（表1）恶臭污染物厂界标准值,二级,新扩改建","西侧场界外3#","臭气浓度","2023-02-24","南","1.6","19.6","100.3","21","20","","无量纲","是","0.05",""]

{"sheet":"周边环境","index":2,"n_rows":46,"n_cols":35,"rows_kept":46,"merged":[[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,1,5],[0,6,1,6],[0,7,1,7],[0,8,1,8],[0,9,0,13],[0,14,0,17],[0,18,0,19],[0,20,0,24],[0,25,0,26],[0,27,1,27],[0,28,1,28],[0,29,1,29],[0,30,1,30],[0,31,1,31],[0,32,1,32],[0,33,1,33],[0,34,1,34],[2,0,45,0],[2,1,45,1]],"flags":["formulas_cached_only"]}
["任务名称","企业名称","名录类别","行业类别","执行标准名称","执行标准条目名称","监测点","监测项目","监测日期","周边环境-环境空气","周边环境-环境空气","周边环境-环境空气","周边环境-环境空气","周边环境-环境空气","周边环境-地表水","周边环境-地表水","周边环境-地表水","周边环境-地表水","周边环境-地下水","周边环境-地下水","周边环境-土壤","周边环境-土壤","周边环境-土壤","周边环境-土壤","周边环境-土壤","周边环境-噪声","周边环境-噪声","折算/浓度/昼间","夜间","上限","下限","单位","是否超标","超标倍数","备注"]
["","","","","","","","","","湿度(%)","气温（℃","气压(kPa)","风速(m/s)","风向","流量(m³/s)","感官描述","有无漂浮物","有无油","井深（m）","水位（m）","采样深度(m)","土壤颜色","土壤水分(%)","利用情况","土壤pH值","声源","风速(m/s)","","","","","","","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW2地下水","硝酸盐","2023-02-24","","","","","","","","","","","","","","","","","","","0.07","","5.0","","mg/L","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW2地下水","铅","2023-02-24","","","","","","","","","","","","","","","","","","","0.002","","0.005","","mg/L","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW2地下水","铜","2023-02-24","","","","","","","","","","","","","","","","","","","<0.05","","0.05","","mg/L","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW2地下水","氟化物","2023-02-24","","","","","","","","","","","","","","","","","","","0.06","","1.0","","mg/L","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW2地下水","硫酸盐","2023-02-24","","","","","","","","","","","","","","","","","","","<8","","150","","mg/L","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW2地下水","总锌","2023-02-24","","","","","","","","","","","","","","","","","","","<0.05","","0.5","","mg/L","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW2地下水","耗氧量（COD法，以O2计）","2023-02-24","","","","","","","","","","","","","","","","","","","0.14","","2.0","","mg/L","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW2地下水","亚硝酸盐","2023-02-24","","","","","","","","","","","","","","","","","","","0.008","","0.1","","mg/L","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW2地下水","镉","2023-02-24","","","","","","","","","","","","","","","","","","","<0.0001","","0.001","","mg/L","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW2地下水","砷","2023-02-24","","","","","","","","","","","","","","","","","","","0.0006","","0.001","","mg/L","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW2地下水","铬（六价）","2023-02-24","","","","","","","","","","","","","","","","","","","<0.004","","0.01","","mg/L","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW2地下水","汞","2023-02-24","","","","","","","","","","","","","","","","","","","<0.00004","","0.0001","","mg/L","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW2地下水","氰化物","2023-02-24","","","","","","","","","","","","","","","","","","","<0.004","","0.01","","mg/L","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","","","GW2地下水","粪大肠菌群","2023-02-24","","","","","","","","","","","","","","","","","","","700","","","","MPN/L","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW2地下水","总硬度","2023-02-24","","","","","","","","","","","","","","","","","","","32","","300","","mg/L","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW2地下水","氯化物","2023-02-24","","","","","","","","","","","","","","","","","","","<10","","150","","mg/L","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW2地下水","挥发性酚类（以苯酚计）","2023-02-24","","","","","","","","","","","","","","","","","","","<0.0003","","0.001","","mg/L","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW2地下水","氨氮","2023-02-24","","","","","","","","","","","","","","","","","","","0.141","","0.1","","mg/L","是","0.41",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW2地下水","锰","2023-02-24","","","","","","","","","","","","","","","","","","","0.08","","0.05","","mg/L","是","0.60",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW2地下水","溶解性总固体","2023-02-24","","","","","","","","","","","","","","","","","","","70","","500","","mg/L","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW2地下水","铁","2023-02-24","","","","","","","","","","","","","","","","","","","0.04","","0.2","","mg/L","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW2地下水","pH值","2023-02-24","","","","","","","","","","","","","","","","","","","6.6","","8.5","6.5","无量纲","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW6地下水","耗氧量（COD法，以O2计）","2023-02-24","","","","","","","","","","","","","","","","","","","2.73","","2.0","","mg/L","是","0.36",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW6地下水","挥发性酚类（以苯酚计）","2023-02-24","","","","","","","","","","","","","","","","","","","<0.0003","","0.001","","mg/L","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW6地下水","铜","2023-02-24","","","","","","","","","","","","","","","","","","","<0.05","","0.05","","mg/L","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW6地下水","氟化物","2023-02-24","","","","","","","","","","","","","","","","","","","0.06","","1.0","","mg/L","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW6地下水","砷","2023-02-24","","","","","","","","","","","","","","","","","","","0.0007","","0.001","","mg/L","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW6地下水","亚硝酸盐","2023-02-24","","","","","","","","","","","","","","","","","","","1.36","","0.1","","mg/L","是","12.60",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW6地下水","总锌","2023-02-24","","","","","","","","","","","","","","","","","","","0.20","","0.5","","mg/L","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW6地下水","汞","2023-02-24","","","","","","","","","","","","","","","","","","","<0.00004","","0.0001","","mg/L","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW6地下水","锰","2023-02-24","","","","","","","","","","","","","","","","","","","17.1","","0.05","","mg/L","是","341.00",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW6地下水","铬（六价）","2023-02-24","","","","","","","","","","","","","","","","","","","<0.004","","0.01","","mg/L","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW6地下水","镉","2023-02-24","","","","","","","","","","","","","","","","","","","0.0008","","0.001","","mg/L","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW6地下水","总硬度","2023-02-24","","","","","","","","","","","","","","","","","","","136","","300","","mg/L","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","","","GW6地下水","粪大肠菌群","2023-02-24","","","","","","","","","","","","","","","","","","","400","","","","MPN/L","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW6地下水","溶解性总固体","2023-02-24","","","","","","","","","","","","","","","","","","","347","","500","","mg/L","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW6地下水","pH值","2023-02-24","","","","","","","","","","","","","","","","","","","6.0","","8.5","6.5","无量纲","是","/",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW6地下水","铅","2023-02-24","","","","","","","","","","","","","","","","","","","0.013","","0.005","","mg/L","是","1.60",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW6地下水","氯化物","2023-02-24","","","","","","","","","","","","","","","","","","","<10","","150","","mg/L","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW6地下水","硝酸盐","2023-02-24","","","","","","","","","","","","","","","","","","","2.08","","5.0","","mg/L","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW6地下水","氨氮","2023-02-24","","","","","","","","","","","","","","","","","","","4.85","","0.1","","mg/L","是","47.50",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW6地下水","氰化物","2023-02-24","","","","","","","","","","","","","","","","","","","<0.004","","0.01","","mg/L","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW6地下水","铁","2023-02-24","","","","","","","","","","","","","","","","","","","0.20","","0.2","","mg/L","否","",""]
["2023年第一季度污染源监测","连平县城环境卫生管理所(连平县城生活垃圾无害化填埋场)","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","GW6地下水","硫酸盐","2023-02-24","","","","","","","","","","","","","","","","","","","117","","150","","mg/L","否","",""]